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Safety Data Sheet according to Regulation (EC) No. 1907/2006 (REACH)


1. IDENTIFICATION OF THE SUBSTANCE/PREPARATION AND OF THE COMPANY/UNDERTAKING
Product name:	STEEL WOOL
Product code nr:	CS6450-56

Company	:	Prime Chemicals
		Northfield Road
 		Rotherham
		S60 1RR

Telephone	:	+44 (0) 1709 377881
Fax	:	+44 (0) 1709 369264

0. Emergency telephone number

Emergency Phone #	:	+44 (0) 1709 377881 (Only manned during normal working hours)

2. HAZARDS IDENTIFICATION
Most important hazards:	none

Specific hazards:	Coarse grades should be cut and not torn as severe cuts can occur.
Do not use near sparks/static or sources of ignition as Fine grades can ignite.
May cause irritation to skin and eyes due to its abrasive nature.

3. COMPOSITION / INFORMATION ON INGREDIENTS
Formula:	Iron – Cas nr: 7439-89-6 99 % w/w Carbon-Cas nr : 7440-44-0 0.15 % w/w Manganese Cas nr : 7439-96-5 0.8 % w/w
Component(s) contributing to the	None according to EC directives. hazard:

4. FIRST AID MEASURES
General advice:	In all cases of doubt, or when symptoms persist, seek medical attention.
Never give anything by mouth to an unconscious person.
In case of accident or if you feel unwell, seek medical advice immediately (show the label where possible).
For symptom description, see item 11.

Inhalation:	Not likely to be a problem – remove to fresh air.
Skin contact:	Wash skin thoroughly with soap and water or a proprietary skin cleaner.
Eye contact:	Immediately wash with copious amounts of water for at least 15 mins. Remove soft contact lenses and seek medical attention.
Ingestion:	If accidentally swallowed seek medical attention.

5. FIRE-FIGHTING MEASURES
Suitable extinguishing media:	Powder, Water spray/mist.

Extinguishing media which must NOT	Do not use a solid water stream as it may scatter and spread fire. be used for safety reasons:

Specific method(s):	Cool closed containers exposed to fire with water spray.
Do not allow run-off from fire fighting to enter drains or water courses.
Specific fire hazard(s):	Concerning product toxicity, see item 11 and about product stability and reactivity
see item 10.
Special protective equipment for	Use a self-contained breathing apparatus and also a protective suit. 
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6. ACCIDENTAL RELEASE MEASURES

Personal precaution(s):	Concerning personal protective equipment to use, see item 8.
Environmental precaution(s):	Concerning disposal elimination after cleaning, see item 13. Method(s) for cleaning up:	Sweep up and dispose of in accordance with local regulations.
Shovel into suitable and closed container for disposal. Dispose as general waste.
7. HANDLING AND STORAGE

Handling

· Precaution(s):	Coarse grades should be cut and not torn as severe cuts can occur.
May cause irritation to skin and eyes due to its abrasive nature.



· Technical condition(s):	Do not use near sparks/static or sources of ignition as
Fine grades can ignite.

· Safe handling advice(s):	Wear heavy duty gloves when handling Storage
· Precaution(s):	Store in a place accessible by authorised persons only.
*Store in a cool dry place away from sources of ignition.
· Keep away from sparks, naked flames and any other sources of ignition.
· Keep dry to avoid rusting.

· Technical condition(s):	Not flammable and waterproof underground retention basin.

· Packaging / tank material:	made of the same material as the supply container, non static

8. EXPOSURE CONTROLS / PERSONAL PROTECTION

Control parameter(s):
· Exposure limit(s):	No data available.

Personal protection equipment:
· Respiratory protection:	No personal breathing protective equipment is normally required.
· Hand protection:	Wear suitable gloves.
· Skin and body protection:	protective clothing
· Eye protection:	safety glasses

9. PHYSICAL AND CHEMICAL PROPERTIES

General information
· Physical state / form:	Fine to Coarse Metal Wool
· Colour:	Grey
· Odour:	None





Important health,safety and environmental information
· PH:	Not applicable.
· Boiling point/range:	Not determined.
· Flash point:	Not applicable.
· Explosion limits:	Not determined.
· Relative density (water = 1):	Not determined
· Viscosity:	Not applicable.
· Water solubility:	Not applicable.
· Fat solubility:	Not applicable.
· Solvent solubility:	Not applicable.


10. STABILITY AND REACTIVITY

Stability:	Stable in use and storage conditions as recommended in item 7. Hazardous decomposition products:	Not Known
11. TOXICOLOGICAL INFORMATION

General information(s):	There is no data available on the product itself. Acute toxicity
· Inhalation:	none
· Skin contact:	none
· Eyes contact:	none
· Ingestion:	none

12. ECOLOGICAL INFORMATION

General information(s):	There is no data available on the product itself. Persistence and degradability:	Product will degrade through oxidation forming iron oxides. Other adverse effects

13. DISPOSAL CONSIDERATIONS

Waste / unused products:	Collect all waste in suitable and labelled containers and dispose according to
local legislation.
Do not dispose of waste into sewer.

Contaminated packaging:	This container is non hazardous and can be disposed of in accordance with local
regulations.
.
Further Information(s):	May be recycled..

14. TRANSPORT INFORMATION

General information(s):	not regulated
UN N°:	Not applicable.

15. REGULATORY INFORMATION

Labelling:	According to European directives on classification, packaging and labelling of dangerous substances
EC number:	Not applicable.
Symbol(s):	None according to EC directives.
R- phrase(s):	None according to EC directives.
S- phrase(s):	None according to EC directives.



16. OTHER INFORMATION

According legislation(s):	This safety data sheet is in compliance with directives and adaptings: 91/155,
67/548, 88/379

Important remarks:	Information in this safety data sheet is based on actual knowledge in our
possession and our experience. It is recommended to pass the information of this safety data sheet, eventually in an appropriated form, to the users.

Uses or/and applications:	wood care

Restrictions:	This information relates to the specific material designated and may not be valid in combination with other product(s).
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