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VERSION - 2

1. IDENTIFICATION OF THE SUBSTANCE/MIXTURE AND OF THE COMPANY/UNDERTAKING

Product name : Acetone

Product Number : ALL

Company : Beecroft & Partners
Northfield Road

Rotherham

S60 1RR

UNITED KINGDOM

Telephone : +441709 375764
Fax : +441709 369264
Emergency Phone # : +441709 375764
E-mail address : Sales@beecroft-science.co.uk
2. HAZARDS IDENTIFICATION

Classification of the substance or mixture

According to Regulation (EC) No1272/2008

Flammable liquids (Category 2)

Eye irritation (Category 2)

Specific target organ toxicity - single exposure (Category 3)

According to European Directive 67/548/EEC as amended.

Highly flammable. Irritating to eyes. Repeated exposure may cause skin dryness or cracking. Vapours may

cause drowsiness and dizziness.

Label elements

Pictogram       [image: image1.png]


[image: image2.png]



Signal word Danger

Hazard statement(s)

H225 Highly flammable liquid and vapour.

H319 Causes serious eye irritation.

H336 May cause drowsiness or dizziness.

EUH066 Repeated exposure may cause skin dryness or cracking.

Precautionary statement(s)

P210 Keep away from heat/sparks/open flames/hot surfaces. - No smoking.

P261 Avoid breathing dust/fume/gas/mist/vapours/spray.

P305 + P351 + P338 IF IN EYES: Rinse cautiously with water for several minutes. Remove

contact lenses, if present and easy to do. Continue rinsing.

Hazard symbol(s)

F Highly flammable

Xi Irritant

R-phrase(s)

R11 Highly flammable.
R36 Irritating to eyes.

R66 Repeated exposure may cause skin dryness or cracking.

R67 Vapours may cause drowsiness and dizziness.

S-phrase(s)

S 9 Keep container in a well-ventilated place.

S16 Keep away from sources of ignition - No smoking.

S26 In case of contact with eyes, rinse immediately with plenty of water and

seek medical advice.

Other hazards - none

3. COMPOSITION/INFORMATION ON INGREDIENTS

Formula : C3H6O

Molecular Weight : 58.08 g/mol

CAS-No. EC-No. Index-No. Classification Concentration

Acetone

67-64-1 200-662-2 606-001-00-8 Flam. Liq. 2; Eye Irrit. 2;

STOT SE 3; H225, H319,

H336, EUH066

F, Xi, R11 - R36 - R66 - R67

-

For the full text of the H-Statements mentioned in this Section, see Section 16.

4. FIRST AID MEASURES

General advice

Consult a physician. Show this safety data sheet to the doctor in attendance.

If inhaled

If breathed in, move person into fresh air. If not breathing give artificial respiration Consult a physician.

In case of skin contact

Wash off with soap and plenty of water. Consult a physician.

In case of eye contact

Rinse thoroughly with plenty of water for at least 15 minutes and consult a physician.

If swallowed

Do NOT induce vomiting. Never give anything by mouth to an unconscious person. Rinse mouth with water.

Consult a physician.

5. FIRE-FIGHTING MEASURES

Suitable extinguishing media

For small (incipient) fires, use media such as "alcohol" foam, dry chemical, or carbon dioxide. For large fires,

apply water from as far as possible. Use very large quantities (flooding) of water applied as a mist or spray;

solid streams of water may be ineffective. Cool all affected containers with flooding quantities of water.

Special protective equipment for fire-fighters

Wear self contained breathing apparatus for fire fighting if necessary.

Further information

Use water spray to cool unopened containers.

6. ACCIDENTAL RELEASE MEASURES

Personal precautions
Use personal protective equipment. Avoid breathing vapors, mist or gas. Ensure adequate ventilation.

Remove all sources of ignition. Evacuate personnel to safe areas. Beware of vapours accumulating to form

explosive concentrations. Vapours can accumulate in low areas.
Environmental precautions

Prevent further leakage or spillage if safe to do so. Do not let product enter drains.

Methods and materials for containment and cleaning up

Contain spillage, and then collect with non-combustible absorbent material, (e.g. sand, earth, diatomaceous

earth, vermiculite) and place in container for disposal according to local / national regulations (see section

13).

7. HANDLING AND STORAGE

Precautions for safe handling

Avoid contact with skin and eyes. Avoid inhalation of vapour or mist.

Keep away from sources of ignition - No smoking. Take measures to prevent the build up of electrostatic

charge.

Conditions for safe storage

Store in cool place. Keep container tightly closed in a dry and well-ventilated place. Containers which are

opened must be carefully resealed and kept upright to prevent leakage.

8. EXPOSURE CONTROLS/PERSONAL PROTECTION

Components with workplace control parameters

Components CAS-No. Value Control

parameters

Update Basis

Acetone 67-64-1 STEL 1,500 ppm

3,620 mg/m3

2005-04-06 UK. EH40 Occupational

Exposure Limits

TWA 500 ppm

1,210 mg/m3

2005-04-06 UK. EH40 Occupational

Exposure Limits

TWA 500 ppm

1,210 mg/m3

2000-06-16 Europe. Commission

Directive 2000/39/EC

establishing a first list of

indicative occupational

exposure limit values

Remarks Indicative

Personal protective equipment

Respiratory protection

Where risk assessment shows air-purifying respirators are appropriate use a full-face respirator with

multi-purpose combination (US) or type AXBEK (EN 14387) respirator cartridges as a backup to

engineering controls. If the respirator is the sole means of protection, use a full-face supplied air

respirator. Use respirators and components tested and approved under appropriate government

standards such as NIOSH (US) or CEN (EU).

Hand protection

The selected protective gloves have to satisfy the specifications of EU Directive 89/686/EEC and the

standard EN 374 derived from it.

Handle with gloves.

Eye protection

Face shield and safety glasses

Skin and body protection

Choose body protection according to the amount and concentration of the dangerous substance at the

work place.

Hygiene measures

Handle in accordance with good industrial hygiene and safety practice. Wash hands before breaks and at

the end of workday.

9. PHYSICAL AND CHEMICAL PROPERTIES

Appearance

Form liquid, clear

Colour colourless

Safety data

pH no data available

Melting point -94 °C - lit.

Boiling point 56 °C at 1,013 hPa - lit.

Flash point -17.0 °C - closed cup

Ignition temperature 465 °C

Lower explosion limit 2 %(V)

Upper explosion limit 13 %(V)

Vapour pressure 533.3 hPa at 39.5 °C

245.3 hPa at 20.0 °C

Density 0.791 g/cm3 at 25 °C

Water solubility completely miscible

Partition coefficient:

n-octanol/water

log Pow: -0.24

10. STABILITY AND REACTIVITY

Chemical stability

Stable under recommended storage conditions.

Conditions to avoid

Heat, flames and sparks.

Materials to avoid

Bases, Oxidizing agents, Reducing agents, Acetone reacts violently with phosphorous oxychloride.

Hazardous decomposition products

Hazardous decomposition products formed under fire conditions. - Carbon oxides

11. TOXICOLOGICAL INFORMATION

Acute toxicity

LD50 Oral - rat - 5,800 mg/kg

Remarks: Behavioral:Altered sleep time (including change in righting reflex). Behavioral:Tremor.

LC50 Inhalation - rat - 8 h - 50,100 mg/m3

LD50 Dermal - guinea pig - 7,426 mg/kg

Skin corrosion/irritation

Skin - rabbit - Mild skin irritation - 24 h

Serious eye damage/eye irritation

Eyes - rabbit - Eye irritation - 24 h

Respiratory or skin sensitization

Chronic exposure may cause dermatitis.

Germ cell mutagenicity

no data available
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Carcinogenicity

This product is or contains a component that is not classifiable as to its carcinogenicity based on its IARC,

ACGIH, NTP, or EPA classification.

IARC: No component of this product present at levels greater than or equal to 0.1% is identified as

probable, possible or confirmed human carcinogen by IARC.

Reproductive toxicity

no data available

Specific target organ toxicity - single exposure

May cause damage to organs.

Specific target organ toxicity - repeated exposure

no data available

Aspiration hazard

no data available

Potential health effects

Inhalation May be harmful if inhaled. May cause respiratory tract irritation. Vapours may

cause drowsiness and dizziness.

Ingestion May be harmful if swallowed.

Skin May be harmful if absorbed through skin. May cause skin irritation. Repeated

exposure may cause skin dryness or cracking.

Eyes Causes eye irritation.

Additional Information

RTECS: AL3150000

12. ECOLOGICAL INFORMATION

Toxicity

Toxicity to fish LC50 - Oncorhynchus mykiss (rainbow trout) - 5,540.00 mg/l - 96 h

Toxicity to daphnia

and other aquatic

invertebrates.

EC50 - Daphnia magna (Water flea) - 13,500.00 mg/l - 48 h

Persistence and degradability

no data available

Bioaccumulative potential

no data available

Mobility in soil

no data available

PBT and vPvB assessment

no data available

Other adverse effects

no data available

13. DISPOSAL CONSIDERATIONS

Product

Burn in a chemical incinerator equipped with an afterburner and scrubber but exert extra care in igniting as

this material is highly flammable. Observe all federal, state, and local environmental regulations. Contact a

licensed professional waste disposal service to dispose of this material.

Contaminated packaging

Dispose of as unused product.

14. TRANSPORT INFORMATION

ADR/RID

UN-Number: 1090 Class: 3 Packing group: II

Proper shipping name: ACETONE

IMDG

UN-Number: 1090 Class: 3 Packing group: II EMS-No: F-E, S-D

Proper shipping name: ACETONE

Marine pollutant: No

IATA

UN-Number: 1090 Class: 3 Packing group: II

Proper shipping name: Acetone

15. REGULATORY INFORMATION

This safety datasheet complies with the requirements of Regulation (EC) No. 1907/2006.

16. OTHER INFORMATION

Text of H-code(s) and R-phrase(s) mentioned in Section 3

EUH066 Repeated exposure may cause skin dryness or cracking.

Eye Irrit. Eye irritation

Flam. Liq. Flammable liquids

H225 Highly flammable liquid and vapour.

H319 Causes serious eye irritation.

H336 May cause drowsiness or dizziness.

STOT SE Specific target organ toxicity - single exposure

F Highly flammable

Xi Irritant

R11 Highly flammable.

R36 Irritating to eyes.

R66 Repeated exposure may cause skin dryness or cracking.

R67 Vapours may cause drowsiness and dizziness.
