
SAFETY DATA SHEET
according to Regulation (EC) No. 1907/2006 (Reach)


SECTION 1: Identification of the substance/mixture and of the company/undertaking
1.1 Product identifiers
Product name	:	Odourless Kerosene
Product Number	:	CO4404-24
Brand	:	Prime Chemicals
Index-No.	:	649-404-00-4
REACH No.	:	A registration number is not available for this substance as the substance
or its uses are exempted from registration, the annual tonnage does not require a registration or the registration is envisaged for a later registration deadline.
CAS-No.	:	8008-20-6
1.2 Relevant identified uses of the substance or mixture and uses advised against
Identified uses	:	Laboratory chemicals, Manufacture of substances
1.3 Details of the supplier of the safety data sheet

PRIME CHEMICALS


Company	:	Prime Chemicals
		Northfield Road
 		Rotherham
		S60 1RR

Telephone	:	+44 (0) 1709 377881
Fax	:	+44 (0) 1709 369264
	
	Emergency telephone number

Emergency Phone #	:	+44 (0) 1709 377881 (Only manned during normal working hours)
[bookmark: _GoBack]


SECTION 2: Hazards identification
2.1 Classification of the substance or mixture
Classification according to Regulation (EC) No 1272/2008
Skin irritation (Category 2), H315 Aspiration hazard (Category 1), H304 Chronic aquatic toxicity (Category 2), H411
For the full text of the H-Statements mentioned in this Section, see Section 16.
Classification according to EU Directives 67/548/EEC or 1999/45/EC
Xn	Harmful	R65
For the full text of the R-phrases mentioned in this Section, see Section 16.
2.2 Label elements
Labelling according Regulation (EC) No 1272/2008
Pictogram	[image: ] Signal word	Danger
Hazard statement(s)
H304	May be fatal if swallowed and enters airways.
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H315	Causes skin irritation.
H411	Toxic to aquatic life with long lasting effects.
Precautionary statement(s)
P273	Avoid release to the environment.
P301 + P310	IF SWALLOWED: Immediately call a POISON CENTER or doctor/
physician.
P331	Do NOT induce vomiting.

Supplemental Hazard Statements
2.3 Other hazards - none

none



SECTION 3: Composition/information on ingredients

	3.1
	Substances
	

	
	CAS-No.	:
	8008-20-6

	
	EC-No.	:
	232-366-4

	
	Index-No.	:
	649-404-00-4


Hazardous ingredients according to Regulation (EC) No 1272/2008
	Component
	Classification
	Concentration

	Kerosine

	CAS-No.	8008-20-6
EC-No.	232-366-4
Index-No.	649-404-00-4
	Skin Irrit. 2; Asp. Tox. 1; Aquatic Chronic 2; H304, H315, H411
	<= 100 %


Hazardous ingredients according to Directive 1999/45/EC
	Component
	Classification
	Concentration

	Kerosine

	CAS-No.	8008-20-6
EC-No.	232-366-4
Index-No.	649-404-00-4
	Xn, R65
	<= 100 %


For the full text of the H-Statements and R-Phrases mentioned in this Section, see Section 16


SECTION 4: First aid measures
4.1 Description of first aid measures General advice
Consult a physician. Show this safety data sheet to the doctor in attendance.
If inhaled
If breathed in, move person into fresh air. If not breathing, give artificial respiration. Consult a physician.
In case of skin contact
Wash off with soap and plenty of water. Consult a physician.
In case of eye contact
Flush eyes with water as a precaution.
If swallowed
Do NOT induce vomiting. Never give anything by mouth to an unconscious person. Rinse mouth with water. Consult a physician.
4.2 Most important symptoms and effects, both acute and delayed
The most important known symptoms and effects are described in the labelling (see section 2.2) and/or in section 11
4.3 Indication of any immediate medical attention and special treatment needed
no data available



SECTION 5: Firefighting measures
5.1 Extinguishing media  Suitable extinguishing media
Use water spray, alcohol-resistant foam, dry chemical or carbon dioxide.
5.2 Special hazards arising from the substance or mixture
Nature of decomposition products not known.
5.3 Advice for firefighters
Wear self contained breathing apparatus for fire fighting if necessary.
5.4 Further information
Use water spray to cool unopened containers.


SECTION 6: Accidental release measures
6.1 Personal precautions, protective equipment and emergency procedures
Use personal protective equipment. Avoid breathing vapours, mist or gas. Ensure adequate ventilation. Remove all sources of ignition. Evacuate personnel to safe areas. Beware of vapours accumulating to form explosive concentrations. Vapours can accumulate in low areas.
For personal protection see section 8.
6.2 Environmental precautions
Prevent further leakage or spillage if safe to do so. Do not let product enter drains. Discharge into the environment must be avoided.
6.3 Methods and materials for containment and cleaning up
Contain spillage, and then collect with an electrically protected vacuum cleaner or by wet-brushing and place in container for disposal according to local regulations (see section 13). Keep in suitable, closed containers for disposal.
6.4 Reference to other sections
For disposal see section 13.


SECTION 7: Handling and storage
7.1 Precautions for safe handling
Avoid contact with skin and eyes. Avoid inhalation of vapour or mist.
Keep away from sources of ignition - No smoking.Take measures to prevent the build up of electrostatic charge.
For precautions see section 2.2.
7.2 Conditions for safe storage, including any incompatibilities
Store in cool place. Keep container tightly closed in a dry and well-ventilated place. Containers which are opened must be carefully resealed and kept upright to prevent leakage.
7.3 Specific end use(s)
A part from the uses mentioned in section 1.2 no other specific uses are stipulated


SECTION 8: Exposure controls/personal protection
8.1 Control parameters
Components with workplace control parameters
Contains no substances with occupational exposure limit values.
8.2 Exposure controls
Appropriate engineering controls
Handle in accordance with good industrial hygiene and safety practice. Wash hands before breaks and at the end of workday.

Personal protective equipment
Eye/face protection
Face shield and safety glasses Use equipment for eye protection tested and approved under appropriate government standards such as NIOSH (US) or EN 166(EU).
Skin protection
Handle with gloves. Gloves must be inspected prior to use. Use proper glove removal technique (without touching glove's outer surface) to avoid skin contact with this product. Dispose of contaminated gloves after use in accordance with applicable laws and good laboratory practices. Wash and dry hands.
The selected protective gloves have to satisfy the specifications of EU Directive 89/686/EEC and the standard EN 374 derived from it.
Full contact
Material: Nitrile rubber
Minimum layer thickness: 0.4 mm Break through time: 480 min
Material tested:Camatril® (KCL 730 / Aldrich Z677442, Size M)
Splash contact Material: Nitrile rubber
Minimum layer thickness: 0.2 mm Break through time: 32 min
Material tested:Dermatril® P (KCL 743 / Aldrich Z677388, Size M)
data source: KCL GmbH, D-36124 Eichenzell, phone +49 (0)6659 87300, e-mail sales@kcl.de, test method: EN374
If used in solution, or mixed with other substances, and under conditions which differ from EN 374, contact the supplier of the CE approved gloves. This recommendation is advisory only and must be evaluated by an industrial hygienist and safety officer familiar with the specific situation of anticipated use by our customers. It should not be construed as offering an approval for any specific use scenario.
Body Protection
Complete suit protecting against chemicals, The type of protective equipment must be selected according to the concentration and amount of the dangerous substance at the specific workplace.
Respiratory protection
Where risk assessment shows air-purifying respirators are appropriate use a full-face respirator with multi-purpose combination (US) or type ABEK (EN 14387) respirator cartridges as a backup to engineering controls. If the respirator is the sole means of protection, use a full-face supplied air respirator. Use respirators and components tested and approved under appropriate government standards such as NIOSH (US) or CEN (EU).
Control of environmental exposure
Prevent further leakage or spillage if safe to do so. Do not let product enter drains. Discharge into the environment must be avoided.


SECTION 9: Physical and chemical properties
9.1 Information on basic physical and chemical properties
a) Appearance	Form: liquid, clear Colour: colourless
b) Odour	no data available
c) Odour Threshold	no data available
d) pH	no data available

e) Melting point/freezing point
f) Initial boiling point and boiling range

no data available

175 - 325 °C at 1,013 hPa

g) Flash point	82 °C - closed cup
h) Evapouration rate	no data available
i) Flammability (solid, gas)  no data available

j) Upper/lower flammability or explosive limits

Upper explosion limit: 5 %(V) Lower explosion limit: 0.7 %(V)

k) Vapour pressure	0.31 hPa at 20 °C
l) Vapour density	no data available
m) Relative density	0.800 g/cm3
n) Water solubility	no data available

o) Partition coefficient: n- octanol/water
p) Auto-ignition temperature
q) Decomposition temperature

no data available no data available no data available

r) Viscosity	no data available
s) Explosive properties	no data available
t) Oxidizing properties	no data available
9.2 Other safety information
Surface tension	32 mN/m at 20 °C


SECTION 10: Stability and reactivity
10.1 Reactivity
no data available
10.2 Chemical stability
Stable under recommended storage conditions.
10.3 Possibility of hazardous reactions
no data available
10.4 Conditions to avoid
Heat, flames and sparks.
10.5 Incompatible materials
Strong oxidizing agents, Strong bases, Strong acids, Amines
10.6 Hazardous decomposition products
Other decomposition products - no data available In the event of fire: see section 5


SECTION 11: Toxicological information
11.1	Information on toxicological effects Acute toxicity
LD50 Oral - rabbit - 2,835 mg/kg
Remarks: Behavioral:Muscle weakness. Lungs, Thorax, or Respiration:Respiratory stimulation. Endocrine:Hypoglycemia.
Skin corrosion/irritation
Skin - rabbit
Result: Irritating to skin. - 24 h (Draize Test)

Serious eye damage/eye irritation
no data available
Respiratory or skin sensitisation
no data available
Germ cell mutagenicity
no data available
Carcinogenicity
IARC:	No component of this product present at levels greater than or equal to 0.1% is identified as probable, possible or confirmed human carcinogen by IARC.
Reproductive toxicity
no data available
Specific target organ toxicity - single exposure
Inhalation - Respiratory system
Specific target organ toxicity - repeated exposure
no data available
Aspiration hazard
May be fatal if swallowed and enters airways.
Additional Information
RTECS: OA5500000
To the best of our knowledge, the chemical, physical, and toxicological properties have not been thoroughly investigated.



SECTION 12: Ecological information
12.1 Toxicity
no data available
12.2 Persistence and degradability
no data available
12.3 Bioaccumulative potential
no data available
12.4 Mobility in soil
no data available
12.5 Results of PBT and vPvB assessment
PBT/vPvB assessment not available as chemical safety assessment not required/not conducted
12.6 Other adverse effects
Toxic to aquatic life with long lasting effects. no data available


SECTION 13: Disposal considerations
13.1	Waste treatment methods Product
This combustible material may be burned in a chemical incinerator equipped with an afterburner and
scrubber. Offer surplus and non-recyclable solutions to a licensed disposal company.
Contaminated packaging
Dispose of as unused product.


SECTION 14: Transport information
14.1 UN number
ADR/RID: 1223	IMDG: 1223	IATA: 1223

14.2 UN proper shipping name ADR/RID:	KEROSENE IMDG:	KEROSENE
IATA:	Kerosene

	14.3
	Transport hazard class(es)
ADR/RID: 3
	
IMDG: 3
	
IATA: 3

	14.4
	Packaging group
ADR/RID: III
	
IMDG: III
	
IATA: III

	14.5
	Environmental hazards
ADR/RID: yes
	
IMDG Marine pollutant: yes
	
IATA: no

	14.6
	Special precautions for user
no data available
	
	


SECTION 15: Regulatory information
This safety datasheet complies with the requirements of Regulation (EC) No. 1907/2006.
15.1 Safety, health and environmental regulations/legislation specific for the substance or mixture

no data available
15.2 Chemical Safety Assessment
For this product a chemical safety assessment was not carried out



SECTION 16: Other information
Full text of H-Statements referred to under sections 2 and 3.
Aquatic Chronic	Chronic aquatic toxicity Asp. Tox.	Aspiration hazard
H304	May be fatal if swallowed and enters airways.
H315	Causes skin irritation.
H411	Toxic to aquatic life with long lasting effects.
Skin Irrit.	Skin irritation
Full text of R-phrases referred to under sections 2 and 3
Xn	Harmful
R65	Harmful: may cause lung damage if swallowed.
Further information
The above information is believed to be correct but does not purport to be all inclusive and shall be used only as a guide. The information in this document is based on the present state of our knowledge and   is applicable to the product with regard to appropriate safety precautions. It does not represent any guarantee of the properties of the product.
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