


Safety Data Sheet according to Regulation (EC) No. 1907/2006 (REACH)



1. Identification of the substance/mixture and of the company/undertaking

1.1 Product identifier

Trade name/designation	n-Pentane 
Product No.	CP1684-16
Substance name	n-Pentane
CAS No.	109-66-0
INDEX no.	601-006-00-1
REACH registration No.	01-2119459286-30
other means of identification
1.2 Relevant identified uses of the substance or mixture and uses advised against
Relevant identified uses	for laboratory use and chemical production.
1.3 Details of the supplier of the safety data sheet

Supplier (manufacturer/importer/only representative/downstream user/distributor)

PRIME CHEMICALS


Company	:	Prime Chemicals
		Northfield Road
 		Rotherham
		S60 1RR

Telephone	:	+44 (0) 1709 377881
Fax	:	+44 (0) 1709 369264
	
	Emergency telephone number

Emergency Phone #	:	+44 (0) 1709 377881 (Only manned during normal working hours)
[bookmark: _GoBack]



2. Hazards identification

2.1 Classification of the substance or mixture

2.1.1 Classification according to Regulation (EC) No. 1272/2008 [CLP]

	hazard classes and hazard categories
	Hazard Statements
	classification procedure
	remark

	Flammable liquid, category 2
	H225
	
	

	Aspiration hazard, category 1
	H304
	
	



2 - 12


	Specific target organ toxicity (single exposure), category 3, narcotic effect
	H336
	
	

	Hazardous to the aquatic environment, chronic, category 2
	H411
	
	




2.1.2 Classification according to Directive 67/548/EEC or 1999/45/EC

	Hazard symbols:
	R-phrases

	F+
	R12

	Xn
	R65

	
	R66

	
	R67

	N
	R51/53




2.2 Label elements

2.2.1 Labelling according to Regulation (EC) No. 1272/2008 [CLP]



[image: ]


Signal word	Danger


Hazard Statements
	H225
	Highly flammable liquid and vapour.

	H304
	May be fatal if swallowed and enters airways.

	H336
	May cause drowsiness or dizziness.

	H411
	Toxic to aquatic life with long lasting effects.

	EUH066
	Repeated exposure may cause skin dryness or cracking.




Precautionary statements
	P210
	Keep away from heat/sparks/open flames/hot surfaces. No smoking.

	P243
	Take precautionary measures against static discharge.

	P280
	Wear protective gloves/protective clothing/eye protection/face protection.

	P273
	Avoid release to the environment.

	P301+P331
	IF SWALLOWED: Do NOT induce vomiting.

	P304+P340
	IF INHALED: Remove victim to fresh air and keep at rest in a position comfortable for breathing.

	P309+P310
	IF exposed or if you feel unwell: Immediately call a POISON CENTER or doctor/physician.




2.2.2 Labelling (67/548/EEC or 1999/45/EC)

Hazard symbols: F+, Xn, N

R-phrases
	R12
	Extremely flammable.

	R65
	Harmful: may cause lung damage if swallowed.

	R66
	Repeated exposure may cause skin dryness or cracking.

	
	




	R67
	Vapours may cause drowsiness and dizziness.

	R51/53
	Toxic to aquatic organisms, may cause long-term adverse effects in the aquatic environment.




S-phrases
	S9
	Keep container in a well-ventilated place.

	S16
	Keep away from sources of ignition - No smoking.

	S29
	Do not empty into drains.

	S33
	Take precautionary measures against static discharges.

	S61
	Avoid release to the environment. Refer to special instructions/safety data sheets.

	S62
	If swallowed, do not induce vomiting: seek medical advice immediately and show this container or label.




2.3 Other hazards

SVHC	No





3. Composition/ Information on ingredients

Molecular formula	H₃C(CH₂)₃CH₃
Molecular weight (g/mol)	72.15 g/mol
CAS No.	109-66-0
EC No	203-692-4
INDEX no.	601-006-00-1
4. First-aid measures
4.1 General information
IF exposed: Immediately call a POISON CENTER or doctor/ physician. If unconscious place in recovery position and seek medical advice. Never give anything by mouth to an unconscious person or a person with cramps. Change contaminated, saturated clothing. Do not leave affected person unattended.
4.2 After inhalation
Immediately call a POISON CENTER or doctor/ physician. Remove casualty to fresh air and keep warm and at rest. If breathing is irregular or stopped, administer artificial respiration.
4.3 In case of skin contact
After contact with skin, wash immediately with plenty of water and soap. Remove contaminated, saturated clothing immediately. In case of skin reactions, consult a physician.
4.4 After eye contact
In case of contact with eyes flush immediately with plenty of flowing water for 10 to 15 minutes holding eyelids apart and consult an ophthalmologist. Protect uninjured eye. Remove contact lenses, if present and easy to do. Continue rinsing.
4.5 After ingestion

Immediately call a POISON CENTER or doctor/ physician. Do not induce vomiting. Rinse mouth thoroughly with water. Give nothing to eat or drink.
4.6 Self-protection of the first aider
First aider: Pay attention to self-protection!
4.7 Information to physician:

Symptoms	No data available
Hazards	No data available
Treatment	No data available





5. Firefighting measures

5.1 Suitable extinguishing media

Water spray ABC-powder Carbon dioxide (CO2) Nitrogen


5.2 Extinguishing media which must not be used for safety reasons:

no restriction


5.3 Special hazards arising from the substance or mixture

In case of fire may be liberated: Carbon dioxide (CO2) Carbon monoxide


5.4 Advice for firefighters

DO NOT fight fire when fire reaches explosives. In case of fire: Wear self-contained breathing apparatus.


5.5 Additional information

Do not allow run-off from fire-fighting to enter drains or water courses. Do not inhale explosion and combustion gases. Use caution when applying carbon dioxide in confined spaces. Carbon dioxide can displace oxygen. Use water spray jet to protect personnel and to cool endangered containers.





6. Accidental release measures

6.1 Personal precautions, protective equipment and emergency procedures

Avoid generation of dust. Do not breathe dust/fume/gas/mist/vapours/spray. Provide adequate ventilation. Remove all sources of ignition. Use personal protection equipment. The accumulation in lowlying or closen rooms can cause increased danger of fire and explosion. The vapour of the product is heavier than air and may accumulate below ground level, in pits, channels and basements in higher concentration. In case of major fire and large quantities: Remove persons to safety.


6.2 Environmental precautions

Do not allow to enter into surface water or drains. Make sure spills can be contained, e.g. in sump pallets or kerbed

areas. Discharge into the environment must be avoided.


6.3 Methods and material for containment and cleaning up

Spilled product must never be returned to the original container for recycling. Prevent spread over a wide area (e.g. by containment or oil barriers). Soak up inert absorbent and dispose as waste requiring special attention.


6.4 Additional information

Clear spills immediately.





7. Handling and storage

7.1 Precautions for safe handling

Avoid: Inhalation. Avoid contact with skin and eyes. Use extractor hood (laboratory). If handled uncovered, arrangements with local exhaust ventilation have to be used. If local exhaust ventilation is not possible or not sufficient, the entire working area must be ventilated by technical means. Keep away from sources of ignition. - No smoking. Usual measures for fire prevention. Take precautionary measures against static discharge.


7.2 Conditions for safe storage, including any incompatibilities

storage temperature	15-25°C


Keep container tightly closed in a cool, well-ventilated place. Keep/Store away from combustible materials.


7.3 Specific end use(s)

No data available





8. Exposure controls / Personal protection

8.1 Control parameters

	Ingredient (Designation)
	Limit value type (country of origin):
	Limit value
	Regulatory information

	n-Pentane
	TWA (EU)
	1000 ppm, 3000 mg/m3
	2006/15/EC




8.2 Appropriate engineering controls

Technical measures and the application of suitable work processes have priority over personal protection equipment. If handled uncovered, arrangements with local exhaust ventilation have to be used.


8.3 Personal protective equipment

Wear suitable protective clothing. When handling with chemical substances, protective clothing with CE-labels including the four control digits must be worn.


8.3.1 Eye / face protection

Eye glasses with side protection DIN-/EN-Norms: DIN EN 166


8.3.2 Skin protection

When handling with chemical substances, protective gloves must be worn with the CE-label including the four control digits. Recommended glove articles DIN-/EN-Norms: DIN EN 374 In the case of wanting to use the gloves again, clean them before taking off and air them well.


By short-term hand contact
Suitable material:	NBR (Nitrile rubber)
Thickness of the glove material	0,12 mm
Breakthrough time (maximum wearing time)	-
Recommended glove articles	VWR 112-0998

By long-term hand contact
Suitable material:	NBR (Nitrile rubber)
Thickness of the glove material	0,38 mm
Breakthrough time (maximum wearing time)	-
Recommended glove articles	VWR 112-3717 / 112-1381


8.3.3 Protective clothing

Wash hands before breaks and after work. Avoid contact with skin and eyes. When using do not eat, drink or smoke. Provide eye shower and label its location conspicuously.


8.3.4 Respiratory protection

Respiratory protection necessary at: aerosol or mist formation


Suitable respiratory protection apparatus:	Full-/half-/quarter-face masks (DIN EN 136/140) Recommendation	VWR 111-0206
Suitable material:	A2B2E2K2P3
Recommendation	VWR 111-0059


8.4 Additional information

Wash hands before breaks and after work. Avoid contact with skin and eyes. When using do not eat, drink or smoke. Provide eye shower and label its location conspicuously.





9. Physical and chemical properties

9.1 Information on basic physical and chemical properties

(a) Appearance
Physical state	liquid
Colour	colourless

(b) Odour	No data available
(c) Odour threshold	No data available

Safety relevant basic data

(d) pH	No data available
(e) Melting point/freezing point	-130°C
(f) Initial boiling point and boiling range	35 to 36 °C (1013 hPa)
(g) Flash point	-40°C
(h) Evaporation rate	No data available
(i) Flammability (solid, gas)	Highly flammable liquid and vapour.
(j) Upper/lower flammability or explosive limits
Lower explosion limit (Vol-%)	1.4
Upper explosion limit (Vol-%)	8
(k) Vapour pressure	400 mmHg (19°C)
(l) Vapour density	2.48 (20°C)
(m) Relative density	0.63 g/cm³ (20°C)
(n) Solubility(ies)
Water solubility (g/l)	0,36 g/l (16°C) at °C:	16
Soluble (g/l) in	No data available
(o) Partition coefficient: n-octanol/water	3.39 (20°C)
(p) Auto-ignition temperature	285°C
(q) Decomposition temperature	No data available
(r) Viscosity
Kinematic viscosity	No data available
Dynamic viscosity	0.25 mPa*s (20°C)
(s) Explosive properties	not applicable
(t) Oxidising properties	not applicable


9.2 Other information

Bulk density	No data available
refraction index	No data available
dissociation constant	No data available
Surface tension	No data available
Henry constant	No data available





10. Stability and reactivity

10.1 Reactivity

Vapours can form explosive mixtures with air.


10.2 Chemical stability

The product is chemically stable under standard ambient conditions (room temperature).


10.3 Possibility of hazardous reactions

Formation of potentially explosive mixtures with: Oxidising agent, strong


10.4 Conditions to avoid

This material is combustible and can be ignited by heat, sparks, flames, or other sources of ignition (e.g. static electricity, pilot lights, or mechanical/electrical equipment).


10.5 Incompatible materials

Rubber articles Plastic articles


10.6 Hazardous decomposition products

No data available


10.7 Additional information

No data available





11. Toxicological information

11.1 Information on toxicological effects

Acute effects

Acute oral toxicity
Effective dose	LD50: Min. 2000 mg/kg
species:	rat
Exposure time remark
source	RTECS

Acute dermal toxicity
Effective dose	No data available
species:	No data available
Exposure time remark  source

Acute inhalation toxicity
Effective dose	No data available
species:	No data available
Exposure time remark  source

Irritant and corrosive effects

Primary irritation to the skin Exposure time
species: Result

Irritation to eyes Exposure time species:
Result

Irritation to respiratory tract Exposure time
species: Result

Sensitisation
In case of skin contact	not sensitising.
After inhalation	not sensitising.

Specific target organ toxicity (single exposure)

May cause drowsiness or dizziness.

Specific target organ toxicity (repeated exposure)

not relevant

CMR effects (carcinogenicity, mutagenicity and toxicity for reproduction)

Carcinogenicity

No indication of human carcinogenicity.

Germ cell mutagenicity/Genotoxicity

No indications of human germ cell mutagenicity exist.

Reproductive toxicity

No indications of human reproductive toxicity exist.

Aspiration hazard

May be fatal if swallowed and enters airways.



11.2 Other adverse effects

No data available


11.3 Additional information

No data available





12. Ecological information

12.1 Ecotoxicity

Acute (short-term) fish toxicity

LC50:	No data available
EC50
species: Exposure time

Chronic (long-term) fish toxicity
LC50:	No data available
EC50
species: Exposure time

Acute (short-term) daphnia toxicity
LC50:	No data available
EC50
species: Exposure time

Chronic (long-term) daphnia toxicity
LC50:	No data available
EC50
species: Exposure time

Acute (short-term) algae toxicity
LC50:	No data available
EC50
species: Exposure time

Chronic (long-term) algae toxicity
LC50:	No data available
EC50
species: Exposure time


12.2 Persistence and degradability

No data available


12.3 Bioaccumulative potential

(o) Partition coefficient: n-octanol/water	3.39 (20°C)


12.4 Mobility in soil

No data available


12.5 Results of PBT assessment

No data available


12.6 Other adverse effects

No data available





13. Disposal considerations

13.1 Waste treatment methods

Appropriate disposal / Product

Dispose according to legislation. Consult the appropriate local waste disposal expert about waste disposal.


Waste code product	16 05 08 (discarded organic chemicals consisting of or containing dangerous substances)


Appropriate disposal / Package



13.2 Additional information

No data available





14. Transport information

14.1 Land transport (ADR/RID)

UN-No.	1265
Proper Shipping Name	PENTANES, LIQUID
Class(es)	3
Classification code:	F1
Packing group	II
Hazard label(s)	3
14.2 Sea transport (IMDG)
UN-No.	1265
Proper Shipping Name	PENTANES, LIQUID
Class(es)	3
Classification code:	F1
Packing group	II
Marine pollutant Segregation group

14.3 Air transport (ICAO-TI / IATA-DGR)

UN-No.	1265
Proper Shipping Name	PENTANES, LIQUID
Class(es)	3
Classification code:	F1
Packing group	II
14.4 Additional information

No data available
15. Regulatory information
15.1 Safety, health and environmental regulations/legislation specific for the substance or mixture
Water hazard class (WGK)	2
15.2 Chemical Safety Assessment
No data available





16. Other information

16.1 Relevant R-, H- and EUH-phrases (Number and full text)

	R12
	Extremely flammable.

	R65
	Harmful: may cause lung damage if swallowed.

	R66
	Repeated exposure may cause skin dryness or cracking.

	R67
	Vapours may cause drowsiness and dizziness.

	R51/53
	Toxic to aquatic organisms, may cause long-term adverse effects in the aquatic environment.




	H225
	Highly flammable liquid and vapour.

	H304
	May be fatal if swallowed and enters airways.

	H336
	May cause drowsiness or dizziness.

	H411
	Toxic to aquatic life with long lasting effects.




EUH066
Repeated exposure may cause skin dryness or cracking.



16.2 Additional information

Indication of changes general update

The above information describes exclusively the safety requirements of the product and is based on our present-day knowledge. The information is intended to give you advice about the safe handling of the product named in this safety data sheet, for storage, processing, transport and disposal. The information cannot be transferred to other products.  In the case of mixing the product with other products or in the case of processing, the information on this safety data sheet is not necessarily valid for the new made-up material.
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